Package com.creditcall.chipdnamobile

# Interface IConnectAndConfigureFinishedListener

public interface IConnectAndConfigureFinishedListener
This interface is used to receive notification of the result after calling method `ChipDnaMobile.connectAndConfigure(Parameters)`.

Author:
  Creditcall Ltd

- ## Method Summary

  Modifier and Type
  Method
  Description
  `void`
  `onConnectAndConfigureFinished(Parameters parameters)`
  Invoked after connect and configure processing is finished.

- ## Method Details

  - ### onConnectAndConfigureFinished

    void onConnectAndConfigureFinished(Parameters parameters)
    Invoked after connect and configure processing is finished.
    Parameters:
      `parameters` - `Parameters` collection which can contain:

      `ParameterKeys.Result` defining whether ChipDna Mobile successfully connected to and configured the PIN pad be retrieved. Value can be either `ParameterValues.TRUE` or `ParameterValues.FALSE`. When the value is `ParameterValues.TRUE` then the PIN pad is ready to process transactions.

      `ParameterKeys.Errors` contains any errors encountered.

      `ParameterKeys.FirmwareUpdateAvailable` defining if a firmware update is available using the values `ParameterValues.TRUE` and `ParameterValues.FALSE`.

      `ParameterKeys.FirmwareUpdateStatus` returned with a serialized `FirmwareUpdateStatus` object. `FirmwareUpdateStatus` can be deserialized using `ChipDnaMobileSerializer.deserializeFirmwareUpdateStatus(java.lang.String)`.